IESNA:LM-63

[ISSUEDATE] 01 November 2021

[TESTLAB] Spectra Lux

[TEST] S2111011-R1

[MANUFAC] Eclairage Luciole

[LUMCAT] Hemingway-30K

[LUMINAIRE] Hemingway Large

[LAMP] (1) Bridgelux BXRC-30G1000-C-73 c/w ERP Power Driver ESS010W-0180-42 @ 120.00V

[\_BURNING] Axial (587 Luminaire Lumens)

[\_REFLECTOR] Round Specular Aluminum Disk

[\_LENS] Cylindrical Acrylic Diffuser

[\_HOUSING] White Painted Cone

[\_NOMINAL COLOR] 3000 K

[\_DRIVE CURRENT] 180 mA

TILT=NONE

1 -1 1.0 73 1 1 1 -2.0000 -2.0000 0.0000

1.0 1 7.22

 0 2.5 5 7.5 10 12.5 15 17.5 20 22.5

 25 27.5 30 32.5 35 37.5 40 42.5 45 47.5

 50 52.5 55 57.5 60 62.5 65 67.5 70 72.5

 75 77.5 80 82.5 85 87.5 90 92.5 95 97.5

 100 102.5 105 107.5 110 112.5 115 117.5 120 122.5

 125 127.5 130 132.5 135 137.5 140 142.5 145 147.5

 150 152.5 155 157.5 160 162.5 165 167.5 170 172.5

 175 177.5 180

 0

 103 104 104 105 106 108 109 110

 111 113 114 115 116 117 117 118

 119 119 119 119 119 119 119 117

 116 114 110 106 100 94 88 79

 59 36 19 6 0 0 0 0

 0 0 0 0 0 0 0 0

 0 0 0 0 0 0 0 0

 0 0 0 0 0 0 0 0

 0 0 0 0 0 0 0 0

 0